BID FORM
Phase 1 Shoreline Restoration
for
Blue Lake CDD
Revised February 16, 2026 Contractor:

ITEM NO.

UNIT PRICE

DESCRIPTION

QUANTITY

UNIT

AMOUNT

I.

Drainage Restoration

1.0

Import Fill

0

CY

$0.00

$0.00

Stabilize all impacted restored areas with sod (match existing species)

2.0

1

LS

$0.00

$0.00

Final Grading (Restore berm/rear swale to design grades)

3.0

1

LS

$0.00

$0.00

4.1

Replace damaged or missing ADS yard drains

0

EA

$0.00

$0.00

Replace damaged or exposed 8" ADS rear yard drainage

4.2

0

LF

$0.00

$0.00

Replace damaged or exposed 12" ADS rear yard drainage

4.3

0

LF

$0.00

$0.00

Replace damaged or exposed 18" ADS rear yard drainage

4.4

0

LF

$0.00

$0.00

5.1

Replace damaged or exposed irrigation main

0

LF

$0.00

$0.00

6.1

Payment and Performance Bond

1

LS

$0.00

$0.00

	Sub-Total Shoreline Restoration	$0.00

1

23218
PARCEL PAVEMENT (SY) LIMEROCK (SY) STABILIZER (SY) SIDEWALK (SY)

2-C
11957.79
11957.79
15111.87
2552.62

2-J
8758.51
8758.51
11040.16
1892.8

TOTAL
20,716.30
20,716.30
26,152.03
4,445.42
-
- 16,269.86
601.76
169.58
-

CURB
2' VALLEY GUTTER (LF) TYPE "F" CURB (LF) TYPE "A" CURB (LF)

9569.88
601.76

6699.98

169.58

ROADWAY SOD (SY) LAKE SOD (SY)
ADA (EA)

2252
3808.45
8

1521.44
5655.42
5

3,773.44
9,463.87
13.00
-
-

25,882.76

WATER
8" PVC DR-18 (LF)
8" PVC DR-14 (LF)
8" GATE VALVE (EA)
10" PVC DR-18 (LF)
10" PVC DR-14 (LF)
10" GATE VALVE (EA) FIRE HYDRANT (EA)

4587.32
233.21
15

3351.74
140.53

7,939.06
373.74
15.00
-
-
- 15.00
-
- 7,844.56
372.94
22.00
-
-
-
-
- 8,011.53
28.00
1.00
1.00
-
- 32.16
- 1.00
-
-
-
- 18.00
- 360.79
84.40
1,276.69
385.00
289.92
1,089.38
1,821.93
415.89
442.37
- 28.00
3.00
-
- 2.00
6.00
10.00
2.00
- 7,588.57
	12,645.45

8,312.80

8

7

IRRIGATION
4" PVC DR-18 (LF)
4" PVC DR-14 (LF)
4" GATE VALVE (EA)
8" PVC DR-18 (LF)
8" PVC DR-14 (LF)
8" GATE VALVE (EA)

4673.88
228.91
15

3170.68
144.03
7

SANITARY
8" SDR-26 (LF)
4' MANHOLE (EA)
6' MANHOLE (EA) LIFT STATION (EA)

4722.73
14
1
1

3288.8
14

FORCEMAIN
4" DR-18 (LF)
4: DR-14 (LF)
4" PLUG VALVE (EA)
8" DR-18 (LF)
8" DR-14 (LF)

32.16

1

DRAINAGE
YARD DRAIN (EA) 30" ADS (LF)
24" ADS (LF)
18" ADS (LF)
12" ADS (LF)
48" RCP (LF)
42" RCP (LF)
36" RCP (LF)
30" RCP (LF)
24" RCP (LF)
18" RCP (LF) JUNCTION BOX (EA) VGI (EA)
TYPE "C" INLET (EA) TYPE "D" INLET (EA) TYPE "9' INLET (EA) 48" HW (EA)
36" HW (EA)
30" HW (EA)
24" HW (EA)

15

3

360.79
84.4
849.84
385
289.92

426.85

1089.38
173.39
202.39
166.75

1648.54
213.5
275.62

18
2

10
1

2

6
1
1

9
1

CENTERLINE (LF) BERM SOD (SY)

4200.27
11809.98

3388.3
835.47

J:\23218\dwg\cost estimate\Quantities_By_Parcel.xlsx